home about us windows insulation costs+grants contact us
home page > windows

### OUR PRODUCTS:

| Combi Alu + Scandinavian, Wooden-Aluminium Windows

| Hi Efficiency Timber - Elite Energy-saving Wooden Windows

| Alu clad - Elite Low maintenance Energy-saving Wooden-Aluminium Windows

| Puro - Architectural Windows Energy-saving Wooden-Aluminium Windows.

| Wooden-Aluminium Balcony Doors Large variety of sizes and finishes

# Combi Alu +

### Scandinavian, Wooden-Aluminium Windows

Combi Alu+ windows are provided with energy-saving triple glazing package, with low-emission glass and argon filled space between the panes.
The overall heat transfer coefficient for the entire window is 1,02 W/m2K.

### The best material and modern structure

The wood the windows are made of is subject to very thorough selection. Timber used to make the windows is carefully dried. All anatomical flaws of the wood - such as knots, burls or twisted fibres - are removed. We make our windows using pine timber.

Standard equipment for the windows includes handles and aluminium drip cap. Depending on the version, two types of fittings can be used:

- scissor version, opening method: awning, tilting, turning vertically and horizontally up to 180°
- hinged version, opening method: side-hinged, awning

Combi Alu+ windows are equipped with mechanisms which prevent uncontrolled opening, and with function of turning the window sash, thus allowing to clean the outer window surface from the inside. Window washing becomes a pleasure.

Combi Alu+ windows are a perfect offer for those who value elegance, simplicity and timeless style, combined with high quality and functionality.

### Warranty

We support our windows with 5 years of limited warranty - get in touch nowto talk to our advisors and find out more.

### Colours

Below is a colour palette offered by KOKOON. Except the presented colours, it is also possible to colour the windows with any colour from the RAL palette.

Due to natural characteristics of timber, some colouristic differences in the wood appearance are acceptable. Moreover, due to various monitor display parameters, the presented sample can differ from actual colours.

### Mullions

Optionally, the windows can be equipped with one of three types of mullions:

## AVAILABLE PANES:

### Low-emission panes

The low emission glass decreases the temperature of the inside pane, which makes the room warm even at low outdoor temperatures.
The heat transfer coefficient for such glazing unit is Us=0,6 W/m2K

### Absorptive panes

Antisol - decrease effects of sunrays, while providing splendid thermal insulation. They are recommended to be installed on southern and south-western facades of buildings.

### Antiburglar panes

The anti-burglar panes are used when special protection of life, health or property is required. The external pane consists of two glued panels, between which several layers of antiburglar foil are placed.

### Safety panes

They prevent injuries in the case of breaking the pane. They are characterized by increased impact strength. They are recommended to be used in sports halls, offices, commercial facilities, public buildings.

### Sound absorbing panes

Sound insulation is ability to muffle noise. Increased sound absorbing power means muffling of noise by at least 38 dB. Windows equipped with glazing units with increased sound insulation are recommended for buildings situated near roads, airports, railway tracks, etc.

### Reflexive panes

Reflexive (mirror) panes decrease effects of sunrays, and the mirroring effect protects privacy of the inhabitants.

## GET IN TOUCH NOW

Your Name |
Your E-mail |
Your Tel. |
Message |

Deansgrange Business Park Blackrock, Co. Dublin T: 01 235 1446, E: info@kokoon.ie, W: www.kokoon.ie