home about us windows insulation costs+grants contact us
home page > windows

### OUR PRODUCTS:

| Combi Alu + Scandinavian, Wooden-Aluminium Windows

| Hi Efficiency Timber - Elite Energy-saving Wooden Windows

| Alu clad - Elite Low maintenance Energy-saving Wooden-Aluminium Windows

| Puro - Architectural Windows Energy-saving Wooden-Aluminium Windows.

| Wooden-Aluminium Balcony Doors Large variety of sizes and finishes

# Hi Efficiency Timber - Elite

### Energy-saving Wooden Windows

Energy-saving wooden windows ELITE 92 are a product which is not only a perfect choice for those who want natural, wooden, energy-saving windows, but also one to emphasize the character of every interior. Thanks to modern technological solutions, they will provide comfort, perfect design and excellent functional properties.
The most important technical parameter which defines the energy-saving level is the overall heat transfer coefficient for the entire window. The lower this factor, the less heat 'escapes' from your home. In the case of wooden pine windows of the ELITE 92 line, this coefficient comes to Uw=0,76 W/m2K.
Another, equally important, parameter is the sound insulation level. Depending on the applied glazing unit, it fluctuates between 32 and 40 dB. This index means that in comparison to the outside surroundings, you can hear this much dB less of noise inside.

### The best material and modern structure

The wood the windows are made of is subject to very thorough selection. Timber used to make the windows is carefully dried. All anatomical flaws of the wood - such as knots, burls or twisted fibres - are removed.
In the ELITE 92 windows, the sash and frame are 92 mm thick and are made of four layers of wood, with appropriately selected alternate ring pattern. We make windows using mainly pine, meranti or oak wood.
Energy efficiency of the ELITE 92 wooden windows results also from their modern construction. An innovative solution is to use 2 groove gasket, an edge gasket, and a gasket on the contact surface between the thermal drip cap and the window frame. The latter prevents both cold air and precipitation water from permeating between the sash and the window frame.

## AVAILABLE PANES:

### Low-emission panes

The low emission glass decreases the temperature of the inside pane, which makes the room warm even at low outdoor temperatures.

The heat transfer coefficient for such glazing unit is Us=0,6 W/m2K

### Absorptive panes

Antisol - decrease effects of sunrays, while providing splendid thermal insulation. They are recommended to be installed on southern and south-western facades of buildings.

### Antiburglar panes

The anti-burglar panes are used when special protection of life, health or property is required. The external pane consists of two glued panels, between which several layers of antiburglar foil are placed.

### Safety panes

They prevent injuries in the case of breaking the pane. They are characterized by increased impact strength. They are recommended to be used in sports halls, offices, commercial facilities, public buildings.

### Sound absorbing panes

Sound insulation is ability to muffle noise. Increased sound absorbing power means muffling of noise by at least 38 dB. Windows equipped with glazing units with increased sound insulation are recommended for buildings situated near roads, airports, railway tracks, etc.

### Reflexive panes

Reflexive (mirror) panes decrease effects of sunrays, and the mirroring effect protects privacy of the inhabitants.

## GET IN TOUCH NOW

Your Name |
Your E-mail |
Your Tel. |
Message |

Deansgrange Business Park Blackrock, Co. Dublin T: 01 235 1446, E: info@kokoon.ie, W: www.kokoon.ie