home about us windows insulation costs+grants contact us
home page > windows

### OUR PRODUCTS:

| Combi Alu + Scandinavian, Wooden-Aluminium Windows

| Hi Efficiency Timber - Elite Energy-saving Wooden Windows

| Alu clad - Elite Low maintenance Energy-saving Wooden-Aluminium Windows

| Puro - Architectural Windows Energy-saving Wooden-Aluminium Windows.

| Wooden-Aluminium Balcony Doors Large variety of sizes and finishes

# Alu clad - Elite

### Low maintenance Energy-saving Wooden-Aluminium Windows

People who build, renovate or expand their houses know, that their choices regarding windows and door will significantly influence the appearance of the entire building. But can windows increase the class and actual value of the building? Owners of ELITE 92-ALU windows will immediately say yes. ELITE 92-ALU windows are a solution dedicated to demanding customers, for whom timeless design, the best materials, safety and excellent thermal parameters are still not enough. With those customers in mind, the ELITE 92-ALU windows are fitted with an aluminium cover plate on the facade side, which makes the beauty of these windows everlasting.
The most important parameter which defines the energy-saving level is the overall heat transfer coefficient for the entire window (Uw). The lower this coefficient is, the less heat the given house loses, which also means lower heating costs. The ELITE92-ALU windows are provided with energy-saving triple-glazing unit, with low-emission glass and argon filled space between the panes. The overall heat transfer coefficient for the entire window is Uw=0,76 W/m2K.
The ELITE92-ALU wooden-aluminium windows provide also high level of sound insulation. Depending on the applied glazing unit, it fluctuates between 32 and 41 dB. The higher this index, the greater the window’s ability to reduce the outdoor noise.

### The best material and modern structure

The wood the windows are made of is subject to very thorough selection. Timber used to make the windows is carefully dried. All anatomical flaws of the wood - such as knots, burls or twisted fibres - are removed.
In the ELITE92-ALU windows, the frame is made of 4 layers of wood and aluminium, and its thickness is no less than 103,5mm. We make windows using mainly pine, meranti or oak wood.
Energy efficiency of the ELITE92-ALU wooden-aluminium windows results also from innovative structural solution, which is undoubtedly a new sealing system. The windows are fitted with two groove gaskets and one edge gasket.
Another innovation which improves thermal insulation parameters of the ELITE92-ALU windows is increasing the depth of seating the glazing unit in the wooden window frame, from 18 to 20mm.

## AVAILABLE PANES:

### Low-emission panes

The low emission glass decreases the temperature of the inside pane, which makes the room warm even at low outdoor temperatures.
The heat transfer coefficient for such glazing unit is Us=0,6 W/m2K

### Absorptive panes

Antisol - decrease effects of sunrays, while providing splendid thermal insulation. They are recommended to be installed on southern and south-western facades of buildings.

### Antiburglar panes

The anti-burglar panes are used when special protection of life, health or property is required. The external pane consists of two glued panels, between which several layers of antiburglar foil are placed.

### Safety panes

They prevent injuries in the case of breaking the pane. They are characterized by increased impact strength. They are recommended to be used in sports halls, offices, commercial facilities, public buildings.

### Sound absorbing panes

Sound insulation is ability to muffle noise. Increased sound absorbing power means muffling of noise by at least 38 dB. Windows equipped with glazing units with increased sound insulation are recommended for buildings situated near roads, airports, railway tracks, etc.

### Reflexive panes

Reflexive (mirror) panes decrease effects of sunrays, and the mirroring effect protects privacy of the inhabitants.

## GET IN TOUCH NOW

Your Name |
Your E-mail |
Your Tel. |
Message |

Deansgrange Business Park Blackrock, Co. Dublin T: 01 235 1446, E: info@kokoon.ie, W: www.kokoon.ie